**Changes in \*.cfg-file for Cheetah and Pegasus:**

Rename micro-channels from "Micro\_u\*" to "HemisphereRegion" (like LA1, LA2, ...).

If DC-Recording:

Copy all macro channels (complete command block of each channel) and rename them to dc\* (like dcAL1, dcAL2, ...).

Change the following command in each of the duplicate channels (all dc-channels) to deactivate the low-cut-filter:

change from:

-SetDspLowCutFilterEnabled %ChanName True

to:

-SetDspLowCutFilterEnabled %ChanName False

**Changes in \*.cfg-file for Pegasus:**

Set the data directory to the wright hard drive:

-SetDataDirectory "F:\"

(probably this command will not exist)

Check if the following two commands exist:

-SetLogFile

-SetDialogVisible "Hardware" false.

If they exist commend them (#). They should only exist in the beginning of the \*.cfg-file.

Check if the following two commands exist:

-SetDiskWriteEnabled

-SetDspHighCutFrequency

If they exist commend them (#). Most likely they will exist in every setting of each channel.